|  |  |
| --- | --- |
| In addition to the manufacturer-related service instructions, we strongly advise the operator/owner to consider the corresponding prescriptions of the European Standard EN1176-7. |  |
| **032622000** | **Mobile sand digger** |
|  | One-time maintenance |  |
| [x]  | Check all screw connections; retighten, if necessary. | once,approx. 4-5 weeks after installation |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Recommended regular inspection and maintenance | once a week | twice per month | once a month | four times a year | twice a year | once a year |
| [x]  | Clean playing sand | [ ]  | [x]  | [ ]  | [ ]  | [ ]  | [ ]  |
| [x]  | Check cleanliness of playing and safety area. Remove any foreign object | [ ]  | [ ]  | [x]  | [ ]  | [ ]  | [ ]  |
| [x]  | Check sheet metal and front edge protection of the bucket for wear, replace, if necessary. | [ ]  | [ ]  | [x]  | [ ]  | [ ]  | [ ]  |
| [x]  | Check tightness of stand construction: stability of (vertical) posts or supports, retighten screw connections, if necessary. | [ ]  | [ ]  | [ ]  | [ ]  | [x]  | [ ]  |
| [x]  | Check further structural components for wear and tightness; retighten, if necessary and replace defective parts. | [ ]  | [ ]  | [ ]  | [ ]  | [x]  | [ ]  |
| [x]  | Check bearings and/or joints for tight fixing and easy-running function, replace or grease, if necessary. | [ ]  | [ ]  | [ ]  | [ ]  | [x]  | [ ]  |

**Please note: The above-mentioned maintenance intervals only have recommendatory character.**

**They must necessarily be adapted to the local circumstances of each playground (frequency of use, social setting, risk and frequency of vandalism etc.).**